大盘菜制作(论坛名aatest)
------------------------------------------------------------------------------------------------------------------------------------------------------
重点：UNAS5安装ISO镜像要使用可选择系统盘的版本
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UNAS5安装完成

将剩余的系统盘空间用起来
直接继续上面的操作
输入root
输入密码yutech
登陆到UNAS5
[image: ]

输入cfdisk,显示
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[image: ]
[image: ]
[bookmark: _GoBack]
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继续输入pvcreate /dev/vda3
（/dev/vda3是刚才的磁盘名字，不同磁盘不同名字，这个要自己看，用cfdisk可以自己看）
[image: ]
继续输入vgcreate devvda3 /dev/vda3
(devvda3是名字，取容易分别是哪个盘就好）
[image: ]
好了。到这里可以用浏览器登陆UNAS了
激活，登陆UNAS
控制中心，逻辑卷管理
[image: ]

如果不小心删除了卷组，只要在命令行里面重新输入vgcreate devvda3 /dev/vda3
就能重新创建
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Please choose whether you want the new partition to be created at the beginning or at the
end of the available space.

Location for the new partition:
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You are editing partition #1 of Virtual disk 1 (vda). No existing file system was
detected in this partition.

Partition settings:

Use as: Ext4 journaling file system
Mount point: /

Mount options: defaults

Label: none

Reserved blocks: 5%

Typical usage: standard

Bootable flag: off

Delete the partition
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This is an overview of your currently configured partitions and mount points. Select a
partition to modify its settings (file system, mount point, etc.), a free space to create
partitions, or a device to initialize its partition table.
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Guided partitioning

Configure software RAID

Configure the Logical Volume Manager
Configure encrypted volumes
Configure iSCSI volumes

Virtual disk 1 (vda) - 42.9 GB Virtio Block Device
#1 primary 20.0 GB f extd /

(1 X ke, SR SWAPEIRS R
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Please choose whether you want the new partition to be created at the beginning or at the
end of the available space.

Location for the new partition:
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You are editing partition #5 of Virtual disk 1 (vda). No existing file sustem was
detected in this partition.

Partition settings:
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This is an overview of your currently configured partitions and mount points. Select a
partition to modify its settings (file system, mount point, etc.), a free space to create
partitions, or a device to initialize its partition table.

<Go Back>

Guided partitioning

Configure software RAID

Configure the Logical Volume Manager
Configure encrypted volumes
Configure iSCSI volumes

Virtual disk 1 (vda) - 42.9 GB Virtio Block Device
#1 primary 20.0 GB f extd /
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If you continue, the changes listed below will be written to the disks.

will be able to make further changes manually.

The partition tables of the following devices are changed:
Virtual disk 1 (vda)

The following partitions are going to be formatted:
partition #1 of Virtual disk 1 (vda) as ext4
partition #5 of Virtual disk 1 (vda) as swap

Hrite the changes to disks?
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Copyright (c) 2007-2021 by Yutech. All rights reserved.

To visit U-NAS Management Center:

ens6: 192.168.100.102
ens6: [feg0::78af:c1ff:fe8S:be?]

For more information, please visit our web site: http://www.u-nas.cn or http://www.u-nas.com

U-NAS-2CNBEOKI login:
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U-NAS 5 (Amalthea) U-NAS-2CNBEOKI ttyl
Copyright (c) 2007-2021 by Yutech. All rights reserved.

To visit U-NAS Management Center:

ens6: 192.168.100.102
ens6: [feB0::78af:c1ff:fed5:be7]

For more information, please visit our web site: http://www.u-nas.cn or http://www.u-nas.com

U-NAS-2CNBEOKI login: root . #HAroot
Password: @ wiyutech
Linux U-NAS-2CNBEOKI 4.19.0-18-amdo4 #1i SMP Debian 4.19.208-1 (2021-03-29) xB86_64

The programs included with the Debian GNU/Linux system are free software;
the exact distribution terms for each program are described in the
individual files in /usr/sharesdoc/*/copuright.

Debian GNU/Linux comes with ABSOLUTELY NO WARRANTY, to the extent
permitted by applicable law.
root@U-NAS-2CNBEDKI: “#  GEXirErnmassktm T




image21.png
a 061504
/dEJ/vdaZ 1951746

ieityasas S Bl

Free SDatQ FREE SPACEQEFRRURMRZSIA) 41017344 BBEEEOV‘E 42868736 20.55. 205628

S Extended

2 1 inuy suap lapi





image22.png
Disk: sdev/vda
Size: 40 GiB, 42349672960 bytes, 83886080 sectors
Label: dos, identifier: Ox3S4cacal
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Disk: /dev/vda
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root@u NAS-2CNBEOKI: “# pvcreate /dev/vda3
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root@U-NAS-2CNBEOKT: “# vgcreate devvda3 /dev/vda3
Volume group devvda3  successfully created] ezsith
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This is an overview of your currently configured partitions and mount points. Select a
partition to modify its settings (file system, mount point, etc.), a free space to create
partitions, or a device to initialize its partition table.
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You have selected an entire device to partition. If you proceed with creating a new
partition table on the device, then all current partitions will be removed.

Note that you will be able to undo this operation later if you wish.

Create new empty partition table on this device?
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